Oasis Pro simulator

|  |
| --- |
| 1.Power : |
| An alkaline 9-volt battery will provide approximately 25-30 hours of operation. |
| (we can set a button as the 9-volt battery once click that the simulator can be provide 25-30 hours of operation ) |

|  |
| --- |
| 2.the battery level when you first turn on the unit; |
| If no session is selected within two (2) minutes; the Oasis Pro will turn off. |
| To turn off the Oasis Pro at any time and hold the power button () until the unit shuts off.  take up to one (1) second if a session is running. |

|  |
| --- |
| 3. ENDING A SESSION |
| All session with soft off: a gradual reduction of the CES stimulus |
| After soft off the unit will power off. |
| To end a session early, press and release the power button (). |
| graph will scroll from 8 to 1 to confirm that soft off is in progress. |

Battery level and battery low warnings as per “Battery Level”

Can be dropdown (combo box ) or frequency bar?(vertical or historical)

|  |
| --- |
| 4: Battery level |
| The battery level is displayed on the graph for a couple of seconds when the Oasis Pro is first turned on. |
| The battery level is also monitored and displayed periodically while the session is running. |
| battery level is getting low, the graph will display two (2) bars and blink. |
| It is recommended that the battery be replaced before running a session if this warning is displayed |
| When the battery level is critically low, the graph will display a single (1) blinking bar. |
| If this warning is displayed when you turn the unit on, replace the battery immediately. |
| If this warning occurs during a session, the session will end early and the battery indicator will continue to blink for a short period of time. |
| The battery must be replaced before the unit can be used again. |

|  |
| --- |
| 5.SELECTING A SESSION |
| The Oasis Pro has four (4) standard session groups（20 minute , 45 minute , 3 hour , and user designed） |
| Each group offers eight (8) sessions. |
| The session number is indicated by the lit number between the intensity and select controls. |
| If no number is lit, then the group has no sessions programmed into it. |
| Press and release the power button () to switch between groups ：lit group icon will change. |
| Press the INT or to highlight a session number. If no sessions are available in a group, no numbers will be lit. |
| The frequency and mode icons associated with the session light up to indicate what frequency range and CES pulse type will be used. |
| Press the select button () to start the highlighted session. The session number will flash and the session will begin after a five (5) second delay |

|  |
| --- |
| Connection Test |
| At the start of each session, the Oasis Pro checks for an electrical connection by entering a test mode |
| The CES Mode light ( or ) will blink. The graph will display the status of the connection. |
| Once a connection has been confirmed, the display will go blank or display a Soft On animation(if resuming or restoring a saved preference). The intensity may be adjusted as soon as the connection test ends. |
| The Oasis Pro will run with either an Okay or Excellent connection  If the connection displayed is Okay then the intensity may have to be turned up higher before it can be felt, or may not be felt at all. |
| If the ear clips are disconnected, the Oasis Pro will pause the session and wait for the ear clips to be reconnected. |
| No Connection (7 and 8 blinking) will display for a couple of seconds, then the graph may scroll up and down indicating that the unit is returning the voltage to a safe testing level; |
| this may take up to 20 seconds (the and lights may turn on as well). |

|  |
| --- |
| ADJUSTING INTENSITY |
| To increase the intensity of the stimulus, press the INT button |
| To decrease the intensity, press the INT button. |
| The graph lights 1 to 8 only show an approximate intensity level. |
| When adjusting intensity, the topmost lit number will blink. |
| Set the intensity so that it can just barely be felt. Setting the intensity too high may result in a skin irritation. A higher intensity will not give better results. |

|  |
| --- |
| SAVING PREFERENCES |
| preferred intensity setting for each session can be saved. |
| Adjust the intensity, then press and hold the Select button for one (1) second |
| The graph will display a short animation. |
| You may continue the session or end it immediately and the Oasis Pro will save your preferred intensity and use it the next time you run that session |
| Can be interrupt the Soft ON process at any time by pressing either INT or . Use saved preferences with caution |

Record:

choose to record a therapy

add to history

session type, duration and intensity level

Replay